{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["例題27 気相PFR","Fogler_5_3","Stream report"],"not_rendered":{"charts":3,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題27 気相PFR","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",1,null,null,null,"定数"]
["xA=","V=",null,null,null,"F=",2.9039999999999999,"m3/s"]
[0.79999999999999916,2.2878265368423945,null,null,null,"cA0=",66.459999999999994,"mol/m3"]
[null,"V'=",null,null,null,"k1=",3.07,"/s"]
["微分方程式→",{"$f":"G2*G3/G7","v":8.5133550488598946},null,null,null,"e=",1]
[null,null,null,null,null,"cA=",{"$f":"G3*(1-A3)/(1+G5*A3)","v":7.3844444444444788}]
["積分区間xA=[a,",0,null,null,null,"-rA=",{"$f":"G4*G6","v":22.670244444444549}]
["b]",0.8]
["積分刻み幅ΔV",2.5000000000000001E-2]
["計算結果"]
["xA","V PFR[m3]"]
[{"$f":"B7","v":0},0,null,null,"←初期値"]
[2.5000000000000001E-2,2.4249455790296099E-2]
[0.05,4.9743144911621087E-2]
[7.4999999999999997E-2,7.6547437975471838E-2]
[9.9999999999999992E-2,0.10473416202494186]
[0.12499999999999999,0.13438121553674739]
[0.15,0.16557327258899757]
[0.17500000000000002,0.19840259217234163]
[0.20000000000000004,0.23296995206543442]
[0.22500000000000006,0.26938573101404933]
[0.25000000000000006,0.30777116840506258]
[0.27500000000000008,0.34825983755803647]
[0.3000000000000001,0.3909993776359072]
[0.32500000000000012,0.43615354064023309]
[0.35000000000000014,0.48390462488446467]
[0.37500000000000017,0.5344563859547159]
[0.40000000000000019,0.58803754219571391]
[0.42500000000000021,0.64490602665886732]
[0.45000000000000023,0.70535418477307843]
[0.47500000000000026,0.76971518195583155]
[0.50000000000000022,0.83837097572642638]
[0.52500000000000013,0.91176233435351284]
[0.55000000000000004,0.99040156676267499]
[0.57499999999999996,1.0748888948100721]
[0.59999999999999987,1.1659337948547805]
[0.62499999999999978,1.2643832362053462]
[0.64999999999999969,1.3712596769984442]
[0.6749999999999996,1.4878131657343432]
[0.69999999999999951,1.6155943400432047]
[0.72499999999999942,1.7565592647469763]
[0.74999999999999933,1.9132243803045996]
[0.77499999999999925,2.0889033714850473]
[0.79999999999999916,2.2880841425991383]

{"sheet":"Fogler_5_3","index":1,"n_rows":29,"n_cols":14,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["解析解"]
["T",1100,"K"]
["p",{"$f":"6*101300","v":607800},"Pa"]
["R",8.3140000000000001]
["CA0(y=1)",{"$f":"B3/B4/B2","v":66.459640912371256},"mol/m3"]
["FA0",193,"mol/s"]
["e",1]
["k1",3.07,"/s"]
["xA",0.8,null,0.8,0.7,0.6,0.5,0.4,0.3,0.2,0.1,0]
["V",{"$f":"($B$6/$B$8/$B$5)*((1+$B$7)*LN(1/(1-B9))-$B$7*B9)","v":2.2880974502845643},"m3",{"$f":"($B$6/$B$8/$B$5)*((1+$B$7)*LN(1/(1-D9))-$B$7*D9)","v":2.2880974502845643},{"$f":"($B$6/$B$8/$B$5)*((1+$B$7)*LN(1/(1-E9))-$B$7*E9)","v":1.6156042208549506},1.1659410026243056,0.83837617749166826,0.58804119658422249,0.3910018095200779,0.23297140174310718,0.10473481393366947,0]
[]
["F",{"$f":"B6/B5","v":2.9040180980585717},"m3/s"]
["F cA0",{"$f":"B12*B5","v":193},"mol/s"]
[]
["COCO<COCO_27_RxnEH.fsd><fogex_5_3>",null,null,null,null,"PFR ReactorタブのSlices for profiles"]
["L",null,null,null,null,0.25,0.5,0.75,1,1.25,1.5,1.75,2,2.2799999999999998]
["D",null,null,null,null,1.1287,1.1287,1.1287,1.1287,1.1287,1.1287,1.1287,1.1287,1.1287]
["V","m3",2.2799999999999998,null,0,{"$f":"(3.14/4)*F17^2*F16","v":0.25001537416250003},{"$f":"(3.14/4)*G17^2*G16","v":0.50003074832500005},0.75004612248750013,1.0000614966500001,1.2500768708125001,1.5000922449750003,1.7501076191375002,2.0001229933000002,2.2801402123620003]
["FA0","mol/s",193,null,null,193,193,193,193,193,193,193,193,193]
["Faout","mol/s",38.81,null,null,152.13,123.9,102.85,86.32,73.09,62.28,53.32,45.83,38.82]
["xA",null,{"$f":"1-C20/C19","v":0.79891191709844556},null,0,{"$f":"1-F20/F19","v":0.21176165803108815},{"$f":"1-G20/G19","v":0.35803108808290152},0.46709844559585501,0.55274611398963736,0.62129533678756477,0.67730569948186525,0.72373056994818652,0.76253886010362693,0.79886010362694304]
[]
["Superficial velocity profile"]
["D","m",1.1287]
["A","m2",{"$f":"(3.14/4)*C24^2","v":1.0000614966500001}]
[null,null,0,20,40,60,80,100]
["V=L","m",0,{"$f":"2.28*D26/100","v":0.45599999999999996},{"$f":"2.28*E26/100","v":0.91199999999999992},1.3679999999999999,1.8239999999999998,2.2799999999999998]
[null,"m/h",10462,13970,15952,17251,18159,18817]
[null,"m/s",{"$f":"C28/3600","v":2.9061111111111111},{"$f":"D28/3600","v":3.8805555555555555},4.431111111111111,4.7919444444444448,5.0441666666666665,5.2269444444444444]

{"sheet":"Stream report","index":2,"n_rows":8,"n_cols":7,"rows_kept":8,"cut":false,"hidden":false,"merged":[[1,5,1,6]]}
[]
[null,"Stream","Feed","Products",null,"PFR"]
[null,"Pressure / [atm]",6,6,null,"Parameter","Value"]
[null,"Temperature / [K]",1100,1100,null,"Ethane conversion",0.80004900000000001]
[null,"Flow rate / [mol / s]",193,347.40899999999999]
[null,"Flow Ethane / [mol / s]",193,38.590600000000002]
[null,"Flow Ethylene / [mol / s]",0,154.40899999999999]
[null,"Flow Hydrogen / [mol / s]",0,154.40899999999999]