{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["例題26 PFR","例題26 液相自触媒反応　CSTRとPFR","Shream report"],"not_rendered":{"charts":3,"images":4,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題26 PFR","index":0,"n_rows":45,"n_cols":13,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",1,null,null,null,"定数"]
["xA=","V=",null,null,null,"F=",5.0000000000000001E-4,"m3/s"]
[0.79999999999999916,3.1288285526502344,null,null,null,"cA0=",500,"mol/m3"]
[null,"V'=",null,null,null,"k=",1.1060000000000001E-6,"m3/mol-s"]
["微分方程式→",{"$f":"G2*G3/G6","v":5.023106288929057},null,null,null,"θC=",0.1]
[null,null,null,null,null,"-rA=",{"$f":"G4*G3^2*(1-A3)*(G5+A3)","v":4.9770000000000168E-2}]
["積分区間xA=[a,",0]
["b]",0.8]
["積分刻み幅ΔV",2.5000000000000001E-2]
["計算結果"]
["xA","V PFR[m3]",null,null,null,null,null,null,null,"V PFR",null,"V CSTR"]
[{"$f":"B7","v":0},0,null,null,"←初期値",null,null,null,null,"xA","V PFR[m3]","xA","V CSTR"]
[2.5000000000000001E-2,0.20422978482584311,null,null,null,null,null,null,null,0,0,0,{"$f":"$G$2*$G$3*L13/($G$4*$G$3^2*(1-L13)*($G$5+L13))","v":0}]
[0.05,0.37544359283589945,null,null,null,null,null,null,null,2.5000000000000001E-2,0.20422978482584311,0.1,{"$f":"$G$2*$G$3*L14/($G$4*$G$3^2*(1-L14)*($G$5+L14))","v":0.50231062889290734}]
[7.4999999999999997E-2,0.52407062830028139,null,null,null,null,null,null,null,0.05,0.37544359283589945,0.2,0.7534659433393609]
[9.9999999999999992E-2,0.65634970141266713,null,null,null,null,null,null,null,7.4999999999999997E-2,0.52407062830028139,0.3,0.96874192715060703]
[0.12499999999999999,0.77631855026636643,null,null,null,null,null,null,null,9.9999999999999992E-2,0.65634970141266713,0.4,1.2055455093429777]
[0.15,0.8867477470652152,null,null,null,null,null,null,null,0.12499999999999999,0.77631855026636643,0.5,1.506931886678722]
[0.17500000000000002,0.98962725442794897,null,null,null,null,null,null,null,0.15,0.8867477470652152,0.6,1.9374838543012141]
[0.20000000000000004,1.0864405681134797,null,null,null,null,null,null,null,0.17500000000000002,0.98962725442794897,0.7,2.6371308016877628]
[0.22500000000000006,1.1783289731982332,null,null,null,null,null,null,null,0.20000000000000004,1.0864405681134797,0.8,4.0184850311432596]
[0.25000000000000006,1.2661950046905086,null,null,null,null,null,null,null,0.22500000000000006,1.1783289731982332]
[0.27500000000000008,1.3507704087337111,null,null,null,null,null,null,null,0.25000000000000006,1.2661950046905086]
[0.3000000000000001,1.4326624445060352,null,null,null,null,null,null,null,0.27500000000000008,1.3507704087337111]
[0.32500000000000012,1.5123864896649308,null,null,null,null,null,null,null,0.3000000000000001,1.4326624445060352]
[0.35000000000000014,1.5903897343994011,null,null,null,null,null,null,null,0.32500000000000012,1.5123864896649308]
[0.37500000000000017,1.6670689543948416,null,null,null,null,null,null,null,0.35000000000000014,1.5903897343994011]
[0.40000000000000019,1.7427843027515584,null,null,null,null,null,null,null,0.37500000000000017,1.6670689543948416]
[0.42500000000000021,1.8178704297081367,null,null,null,null,null,null,null,0.40000000000000019,1.7427843027515584]
[0.45000000000000023,1.8926458542250129,null,null,null,null,null,null,null,0.42500000000000021,1.8178704297081367]
[0.47500000000000026,1.967421278741889,null,null,null,null,null,null,null,0.45000000000000023,1.8926458542250129]
[0.50000000000000022,2.0425074056984673,null,null,null,null,null,null,null,0.47500000000000026,1.967421278741889]
[0.52500000000000013,2.1182227540551839,null,null,null,null,null,null,null,0.50000000000000022,2.0425074056984673]
[0.55000000000000004,2.1949019740506244,null,null,null,null,null,null,null,0.52500000000000013,2.1182227540551839]
[0.57499999999999996,2.2729052187850947,null,null,null,null,null,null,null,0.55000000000000004,2.1949019740506244]
[0.59999999999999987,2.3526292639439905,null,null,null,null,null,null,null,0.57499999999999996,2.2729052187850947]
[0.62499999999999978,2.4345212997163146,null,null,null,null,null,null,null,0.59999999999999987,2.3526292639439905]
[0.64999999999999969,2.5190967037595171,null,null,null,null,null,null,null,0.62499999999999978,2.4345212997163146]
[0.6749999999999996,2.6069627352517926,null,null,null,null,null,null,null,0.64999999999999969,2.5190967037595171]
[0.69999999999999951,2.6988511403365458,null,null,null,null,null,null,null,0.6749999999999996,2.6069627352517926]
[0.72499999999999942,2.7956644540220763,null,null,null,null,null,null,null,0.69999999999999951,2.6988511403365458]
[0.74999999999999933,2.8985439613848101,null,null,null,null,null,null,null,0.72499999999999942,2.7956644540220763]
[0.77499999999999925,3.0089731581836587,null,null,null,null,null,null,null,0.74999999999999933,2.8985439613848101]
[0.79999999999999916,3.1289420070373577,null,null,null,null,null,null,null,0.77499999999999925,3.0089731581836587]
[null,null,null,null,null,null,null,null,null,0.79999999999999916,3.1289420070373577]

{"sheet":"例題26 液相自触媒反応　CSTRとPFR","index":1,"n_rows":49,"n_cols":14,"rows_kept":49,"cut":false,"hidden":false,"merged":[]}
["橋本健治：反応工学 p. 89 例題5.6 酢酸メチルの加水分解反応",null,null,null,null,null,null,null,null,null,null,"τ",2475,"s"]
[null,null,"Methyl acetate","Water","Acetic acid","Methanol",null,null,null,null,null,"V",{"$f":"M1*G8","v":1.2375},"m3"]
[null,null,"(A)","(B)","(C)","(D)"]
["供給","mol/s",0.24999015795717086,26.75326564287106,2.4995193900625247E-2,0]
["MW","kg/kmol",74.078999999999994,18.015000000000001,60.05,32.04]
["density","kmol/m3",12.45,55.91,17.670000000000002,25.065999999999999]
["F0i","m3/s",{"$f":"(C4*0.001)/C6","v":2.0079530759612119E-5},{"$f":"(D4*0.001)/D6","v":4.7850591384137117E-4},{"$f":"(E4*0.001)/E6","v":1.4145553990167089E-6},{"$f":"(F4*0.001)/F6","v":0}]
["F0 =F","m3/s",null,null,null,null,{"$f":"SUM(C7:F7)","v":5.0000000000000001E-4}]
["c0i","mol/m3",{"$f":"C4/$G$8","v":499.9803159143417},{"$f":"D4/$G$8","v":53506.531285742116},49.990387801250492,0]
[]
["k",null,1.1060000000000001E-6]
["cA0",null,{"$f":"C9","v":499.9803159143417}]
["θc",null,{"$f":"E9/C9","v":9.998471181776486E-2}]
["xA",null,0.45]
["-rA=kcAcC","mol/m3-s",{"$f":"C11*C12^2*(1-C14)*(C13+C14)","v":8.3632339756254462E-2}]
[]
[]
["Levenspiel プロット"]
[null,"-rA","F cA0/-rA"]
["xA","mol/s-m3","m3"]
[0,{"$f":"$C$11*$C$12^2*(1-A21)*($C$13+A21)","v":2.7643596133417943E-2},{"$f":"$G$8*$C$12/B21","v":9.0433298457490263}]
[0.05,{"$f":"$C$11*$C$12^2*(1-A22)*($C$13+A22)","v":3.9394132243662366E-2},6.3458729439938022]
[0.1,4.9762277204757815E-2,5.0236880625163405]
[0.15,5.8748031016704283E-2,4.2552942393267479]
[0.2,6.6351393679501769E-2,3.7676700381713526]
[0.25,7.2572365193150259E-2,3.4447018130362133]
[0.3,7.7410945557649782E-2,3.2293903162699027]
[0.35,8.0867134773000324E-2,3.0913690544237857]
[0.4,8.2940932839201884E-2,3.0140745877771642]
[0.45,8.3632339756254462E-2,2.9891565713187558]
[0.5,8.2941355524158045E-2,3.0140592274785898]
[0.55000000000000004,8.0867980142912646E-2,3.0913367381673158]
[0.6,7.7412213612518294E-2,3.2293374170706453]
[0.65,7.2574055932974946E-2,3.4446215626703682]
[0.7,6.6353507104282616E-2,3.7675500341569119]
[0.75,5.8750567126441292E-2,4.2551105493015786]
[0.8,4.9765235999450985E-2,5.0233893788814497]
[0.85,3.9397513723311732E-2,6.3453282791611869]
[0.9,2.7647400298023456E-2,9.0420855220533323]
[]
["CSTRとPFRの組み合わせ"]
["V CSTR"]
["xA",0.45]
["V CSTR",{"$f":"G8*C12*B43/($C$11*$C$12^2*(1-B43)*($C$13+B43))","v":1.3451204570934401},"m3"]
["V PFR","(微分方程式解法シートより）"]
["xA 1",0.45]
["xA 2",0.8]
["V PFR",1.236,"m3"]
["合計V",{"$f":"B44+B48","v":2.5811204570934398},"m3"]

{"sheet":"Shream report","index":2,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[[6,6,6,7],[1,6,1,7]]}
[]
[null,"Stream","Feed",2,"Products",null,"CSTR"]
[null,"Pressure / [MPa]",0.1013,0.1013,0.1013,null,"Parameter","Value"]
[null,"Temperature / [°C]",25,25,25,null,"Reactor volume / [m³]",1.345]
[null,"Flow rate / [mol / s]",27.024999999999999,27.024999999999999,27.024999999999999,null,"Methyl acetate conversion",0.45152500000000001]
[null,"Flow Methyl acetate / [mol / s]",0.25,0.13711899999999999,4.9586400000000003E-2]
[null,"Flow Water / [mol / s]",26.75,26.6371,26.549600000000002,null,"PFR"]
[null,"Flow Acetic acid / [mol / s]",2.5000000000000001E-2,0.137881,0.225414,null,"Parameter","Value"]
[null,"Flow Methanol / [mol / s]",0,0.112881,0.20041400000000001,null,"Length / [m]",1.236]
[null,null,null,null,null,null,"Methyl acetate conversion",0.63836899999999996]