{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["例題30 非等温気相PFR","Stream report"],"not_rendered":{"charts":4,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"例題30 非等温気相PFR","index":0,"n_rows":61,"n_cols":23,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
["微分方程式数",2,null,null,null,"定数",null,null,"T0=",1035,"K",null,"<COCO_29_PFRHeat.fsd>",null,null,null,null,null,"D=",2.6689999999999998E-2,"m",0,1100]
["V=","xA=","T=",null,null,"FA0=",3.7600000000000001E-2,"mol/s","Ta=",1100,"K",null,"V","L","T",null,null,"xA","a=(4/D)=",{"$f":"4/T1","v":149.86886474334958},"/m",1E-3,1100]
[9.9999999999999937E-4,0.49944410268748946,1019.958965306942,null,null,"ΣFi=",{"$f":"G2*(1+B3)","v":5.6379098261049601E-2},"mol/s","ΔrH=",80770,"J/mol ",null,"m3","m","C","K ",null,"Acetone","L=",1.79,"m"]
[null,"xA'=","T'=",null,null,"cA0=",18.8,"mol/m3","U=",110,"J/m2-s-K",null,0,0,761.8,{"$f":"O4+273.15","v":1034.9499999999998},0.13500000000000001,{"$f":"1-Q4/$Q$4","v":0},"V=",{"$f":"T3*(3.14/4)*T1^2","v":1.000967173915E-3},"m3"]
["微分方程式→",{"$f":"G6/G2","v":372.3683596617563},{"$f":"(-J5*(C3-J2)+(-G6)*J3)/(G3*J6)","v":20280.206077217372},null,null,"k=",{"$f":"3.58*EXP(34222*(1/J1-1/C3))","v":2.1984814993236679},"1/s","Ua=",{"$f":"J4*T2","v":16485.575121768452},"J/m3-s-K",null,1E-4,0.17882704314857012,736.4,{"$f":"O5+273.15","v":1009.55},0.122,{"$f":"1-Q5/$Q$4","v":9.6296296296296324E-2}]
[null,null,null,null,null,"-ra=",{"$f":"G5*G4*(1-B3)*(J1/C3)/(1+B3)","v":14.001050323282037},"mol/m3-s","Cp=",165,"J/mol-K",null,2.0000000000000001E-4,0.35765408629714024,733.1,1006.25,0.114,0.15555555555555556]
["積分区間V=[a,",0,null,null,null,null,null,null,null,null,null,null,2.9999999999999997E-4,0.53648112944571036,733.8,1006.9499999999999,0.1075,0.20370370370370372]
["b]",1E-3,null,null,null,null,null,null,null,null,null,null,4.0000000000000002E-4,0.71530817259428048,735.5,1008.65,0.1012,0.25037037037037047]
["積分刻み幅ΔV",5.0000000000000002E-5,null,null,null,null,null,null,null,null,null,null,5.0000000000000001E-4,0.8941352157428506,737.6,1010.75,9.5000000000000001E-2,0.29629629629629628]
["計算結果",null,null,null,null,null,null,null,null,null,null,null,5.9999999999999995E-4,1.0729622588914207,739.7,1012.85,8.8999999999999996E-2,0.34074074074074079]
["V[m3]","xA","T[K]",null,null,null,null,null,null,null,null,null,6.9999999999999999E-4,1.2517893020399908,741.9,1015.05,8.3199999999999996E-2,0.38370370370370377]
[0,0,1035,null,null,null,null,null,null,null,null,null,8.0000000000000004E-4,1.430616345188561,744.1,1017.25,7.7499999999999999E-2,0.42592592592592593]
[5.0000000000000002E-5,6.0226919516342486E-2,1016.1659899004264,null,null,null,null,null,null,null,null,null,8.9999999999999998E-4,1.6094433883371311,746.3,1019.4499999999999,7.1999999999999995E-2,0.46666666666666679]
[1E-4,9.7773323571920506E-2,1009.8914369896082,null,null,null,null,null,null,null,null,null,1E-3,1.7882704314857012,748.5,1021.65,6.6000000000000003E-2,0.51111111111111107]
[1.5000000000000001E-4,0.12839467717028916,1007.3515364063828]
[2.0000000000000004E-4,0.15577266917458268,1006.4562359131554]
[2.5000000000000006E-4,0.18133768244696738,1006.3910551164855]
[3.0000000000000008E-4,0.20576093997860298,1006.7756764356499,null,null,null,null,null,null,null,null,null,"断熱条件 U=0"]
[3.500000000000001E-4,0.22939143815887711,1007.4145147258258,null,null,null,null,null,null,null,null,null,"V","L","T",null,null,"xA"]
[4.0000000000000013E-4,0.25242237896786113,1008.2009661626581,null,null,null,null,null,null,null,null,null,"m3","m","C","K ",null,"Acetone"]
[4.5000000000000015E-4,0.27496525571464581,1009.0746907281296,null,null,null,null,null,null,null,null,null,0,0,761.8,{"$f":"O21+273.15","v":1034.9499999999998},0.13253599999999999,{"$f":"1-Q21/$Q$4","v":1.8251851851851963E-2}]
[5.0000000000000012E-4,0.29708631588999801,1010.0006474357169,null,null,null,null,null,null,null,null,null,1E-4,0.17882704314857012,722.2,{"$f":"O22+273.15","v":995.35},0.124,{"$f":"1-Q22/$Q$4","v":8.1481481481481599E-2}]
[5.5000000000000003E-4,0.31882576320601458,1010.9581287083225,null,null,null,null,null,null,null,null,null,2.0000000000000001E-4,0.35765408629714024,706.7,979.85,0.12,0.11111111111111116]
[5.9999999999999995E-4,0.34020835986110504,1011.9347639826302,null,null,null,null,null,null,null,null,null,2.9999999999999997E-4,0.53648112944571036,696.99,970.14,0.11749999999999999,0.12962962962962976]
[6.4999999999999986E-4,0.36124948602485779,1012.9231322921056,null,null,null,null,null,null,null,null,null,4.0000000000000002E-4,0.71530817259428048,689.95,963.1,0.11559999999999999,0.14370370370370378]
[6.9999999999999978E-4,0.38195869541170008,1013.9188004126514,null,null,null,null,null,null,null,null,null,5.0000000000000001E-4,0.8941352157428506,684.45,957.6,0.114,0.15555555555555556]
[7.4999999999999969E-4,0.40234184607038787,1014.9191637319996,null,null,null,null,null,null,null,null,null,5.9999999999999995E-4,1.0729622588914207,679.9,953.05,0.1129,0.1637037037037038]
[7.999999999999996E-4,0.42240240012716779,1015.9227499155395,null,null,null,null,null,null,null,null,null,6.9999999999999999E-4,1.2517893020399908,676.11,949.26,0.1119,0.17111111111111121]
[8.4999999999999952E-4,0.44214222902064337,1016.9287945704618,null,null,null,null,null,null,null,null,null,8.0000000000000004E-4,1.430616345188561,672.8,945.94999999999993,0.111,0.17777777777777781]
[8.9999999999999943E-4,0.46156211952640636,1017.9369793873827,null,null,null,null,null,null,null,null,null,8.9999999999999998E-4,1.6094433883371311,669.9,943.05,0.11,0.18518518518518523]
[9.4999999999999935E-4,0.48066209611384347,1018.947268715094,null,null,null,null,null,null,null,null,null,1E-3,1.7882704314857012,667.3,940.44999999999993,0.1095,0.18888888888888899]
[9.9999999999999937E-4,0.4994416291214468,1019.959806517604]
[]
[]
[]
[]
[]
[]
[]
[]
[0,0,1035]
[5.0000000000000002E-5,5.4723171777108594E-2,1008.8512861330541]
[1E-4,8.2098903128266662E-2,996.30654153180251]
[1.5000000000000001E-4,0.10064676333984736,987.98688936942369]
[2.0000000000000004E-4,0.11469367908845554,981.77898772921208]
[2.5000000000000006E-4,0.12600224832611323,976.83786663192734]
[3.0000000000000008E-4,0.13546723581741626,972.74027734818708]
[3.500000000000001E-4,0.14360583100336319,969.24413253231637]
[4.0000000000000013E-4,0.15074413497746278,966.19811046080554]
[4.5000000000000015E-4,0.15710105948899328,963.50137903110465]
[5.0000000000000012E-4,0.16283069960729468,961.08341850821523]
[5.5000000000000003E-4,0.16804563863469146,958.89300102248365]
[5.9999999999999995E-4,0.17283063723413719,956.89175666779056]
[6.4999999999999986E-4,0.17725110707019009,955.05021254990493]
[6.9999999999999978E-4,0.18135858556237935,953.34524622241793]
[7.4999999999999969E-4,0.18519440159545025,951.75838823441575]
[7.999999999999996E-4,0.18879220525737767,950.27465552898491]
[8.4999999999999952E-4,0.19217975949638483,948.88172835987029]
[8.9999999999999943E-4,0.19538023792200418,947.56935619804244]
[9.4999999999999935E-4,0.19841318360178631,946.32892027852517]
[9.9999999999999937E-4,0.20129522986048898,945.15310575718001]

{"sheet":"Stream report","index":1,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Stream","Feed","Products"]
[null,"Pressure / [kPa]",162,161.976]
[null,"Temperature / [K]",1035,1021.68]
[null,"Flow rate / [mol / s]",3.7600000000000001E-2,5.6660700000000001E-2]
[null,"Flow Acetone / [mol / s]",3.7600000000000001E-2,1.8539300000000002E-2]
[null,"Mole frac Acetone",1,0.32719799999999999]
[null,"Mole frac Methane",0,0.33640100000000001]
[null,"Mole frac Ketene",0,0.33640100000000001]